**Reporting protocol**

This protocol aims to check some input data and model results of two scenarios; one with and another without time slices.

The following parts should be implemented and checked:

1. **Electricity demand** in each region and model year, for industry and buildings.
2. **Capacity factor** of renewables in each time slices; and comparing the yearly equivalent of them with the yearly capacity factor in the old model (= the model without time slices), for one or a group of technologies, in each model region and model year.
3. **Electricity generation** of technologies (e.g., renewables) in two models, for each region and model year.
4. **Installed capacity** of technologies in two models, for each region and year.